# iac_layer_extended_impl

A transfer function that is used to mimic the synchronization bug in the SCM simulator for the decision layer. The “unshunted” channel is ignored and lateral inhibition is implemented internally — with SCM's additional inhibition term multiplying by own state — based on the most recently updated state of the preceding node.

# Parameters

    parameter		default_value
    decay			0
    rate			1
    max_act			1
    min_act			0
    extra_inhibition	0